Back to Table of Contents

# Stamp Profile Tool

## Launch the Tool

1. Open the Profile Builder dialog.
2. Click the Stamp Profile Tool Button

## Stamp the Selected Profile

After launching the tool, a component will be created of the current proilfe.
Click anywhere in your model to place the component.
The component will automatically align to any face in your model.

- Previous Page: Importing PLB files
- Page 8 of 37
- Next Page: Build Tool