Back to Table of Contents

# Saving Profiles

## Choose the Default Profile Attributes

For this profile, the placement point was changed to 'Top-Left' and the Y Offset was changed to -1"

## Click the 'Save Profile' Button

## Choose where to save the Profile

1. Select a Folder to save the Profile.
2. Choose a Name for the Profile. You may wish to use a name that also includes important attrubtes of the Profile.
3. Click 'Save' to save the profile as a SKP file.

## Congratulations! You just saved a Profile!

- Previous Page: Create a Profile from a Polyline
- Page 3 of 37
- Next Page: Loading Profiles