Back to Table of Contents

# PMPI within a Tool

## Profile Member Path Inferencing

In order to connect Profile Members precisely, use PMPI.

Activate PMPI within a tool by hovering the cursor over a Profile Member and presssing the CTRL button (Windows) or OPTION (Mac).

## Replace a Profile Member with its Path

After activating PMPI, the Profile Member will be temporarily replaced by its path so you can inference to the path.

In the example above, PMPI is used to connect two pipes at their centerlines.

## Congratulations! You just used PMPI!

## PMPI with Assemblies

PMPI can be used when building an Assembly.

## Congratulations! You just used PMPI when building an Assembly!

A common use of PMPI is to make it easier to draw a closed path.

- Previous Page: Quantity Reference
- Page 34 of 37
- Next Page: PMPI outside a Tool