Back to Table of Contents

# Build Assembly Tool

## Build an Assembly

Now that you have created an assembly, it is time to build it!
1. Click the 'Build Assembly' Button.
2. Click a point in the model to define the start of the assembly.
3. Continue clicking points to define the path of the assembly.

To complete the assembly:
Press ESC or RETURN or ENTER
OR
Right-click and select 'Finish'
OR
Create a closed path for the Assembly.

## Congratulations! You just built an Assembly!

## Modifier Keys

Arrows Keys = Lock Axis
SHIFT = Lock Inference
CTRL / OPTION = Profile Member or Assembly path Inferecing (PMPI)
BACKSPACE = Undo the last path point

You can also enter values in the Measurements box to draw precisely.

- Previous Page: Loading Assemblies
- Page 19 of 37
- Next Page: Build Assembly along Path